(footprint "Littelfuse 0157004.DR" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -2.54 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.1)))
    (tstamp b07b3668-3bdd-4cce-a1d9-91cfad350c72)
  )
  (fp_text value "Littelfuse 0157004.DR" (at 0 0 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp aa8a6308-241c-4e34-825a-ffa15bc7b8b0)
  )
  (fp_text user "${REFERENCE}" (at 0 1.27 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c82b36e5-7445-4350-bec5-b593c130ae72)
  )
  (fp_line (start -3.25 -1.85) (end -3.25 -1.6)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp f2411688-ef36-4d76-bd58-333937e2f46e))
  (fp_line (start -3.25 -1.85) (end 3.25 -1.85)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp aed64438-82ac-4c05-a169-7f50580e4348))
  (fp_line (start -3.25 1.85) (end -3.25 1.6)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 0cfa684e-55df-4752-86c2-a19883fc42e3))
  (fp_line (start -3.25 1.85) (end 3.25 1.85)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 9f2ebdd7-092c-44bc-8b90-c1ea8a23c910))
  (fp_line (start 3.25 -1.85) (end 3.25 -1.6)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 86e33b7e-e43a-46bd-a6e8-b0c5093a92db))
  (fp_line (start 3.25 1.85) (end 3.25 1.6)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 873609c8-99eb-4dcb-bf9f-4f472fae2d64))
  (pad "1" smd rect (at -2.43 0) (size 2.4 3) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 72c80abb-302e-4b23-a1b6-1234d61efc1d))
  (pad "2" smd rect (at 2.43 0) (size 2.4 3) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp bb582639-61cb-4e25-9980-4823321cc4f9))
)
