(footprint "Bourns SRP1050WA-680M" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 0 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.1)))
    (tstamp 3750fa3d-dbb0-4f91-b1c1-8e0b8a07804e)
  )
  (fp_text value "Bourns SRP1050WA-680M" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp ac506e7a-0d8b-4af6-ad5c-20029d41bc11)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b108eccc-7c9f-4f77-b050-deef7b6c60ae)
  )
  (fp_line (start -5 -5) (end 5 -5)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 57391630-80b5-40e2-9edf-960baf25cbc8))
  (fp_line (start -5 -3) (end -5 -5)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 434727d8-c0d8-403c-8a12-7f6b28623291))
  (fp_line (start -5 3) (end -5 5)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 3a65129c-f15d-45e1-b9dd-8b4c2dd92730))
  (fp_line (start -5 5) (end 5 5)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 0201fb3e-e798-4b8b-83f2-85dcae9164ce))
  (fp_line (start 5 -5) (end 5 -3)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp a5aaf02d-b4ba-4571-ac55-2eb921bf276f))
  (fp_line (start 5 5) (end 5 3)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp be07bc35-eeef-41a2-aa72-f297e5905c01))
  (pad "1" smd rect (at -4.45 0) (size 3.4 5) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 4be3a0e5-a49c-4d5d-be77-9f55e62a6b4a))
  (pad "2" smd rect (at 4.45 0) (size 3.4 5) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 9a270cde-fcf3-4fd3-868e-6c6d19c489b5))
)
