(footprint "L201011MS02Q" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 0 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.1)))
    (tstamp 53c3d997-60f0-4a19-9adb-27c634e20aa6)
  )
  (fp_text value "L201011MS02Q" (at 0 8.2 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 742239ca-fcda-4233-b471-4191bdcaf381)
  )
  (fp_text user "${REFERENCE}" (at 0 6.7 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp fadbd9a7-6976-466c-8d0d-9d1487c59d93)
  )
  (fp_rect (start -9.6 5.4) (end 9.5 -5.4)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.SilkS") (tstamp a55de2a3-7d3b-4c10-8fab-26b6e7a9b933))
  (pad "1" thru_hole circle (at -4.6 -2.85) (size 3 3) (drill 1.65) (layers "*.Cu" "*.Mask") (tstamp ca18352b-82f5-4efd-b9f3-5c7dce1b224e))
  (pad "2" thru_hole circle (at 0 -2.85) (size 3 3) (drill 1.65) (layers "*.Cu" "*.Mask") (tstamp b0cf7ec5-046b-4276-be43-8a62d24768aa))
  (pad "3" thru_hole circle (at -4.6 2.85) (size 3 3) (drill 1.65) (layers "*.Cu" "*.Mask") (tstamp 67d36222-f4b8-4eac-b1e3-3b014158df43))
  (pad "4" thru_hole circle (at 0 2.85) (size 3 3) (drill 1.65) (layers "*.Cu" "*.Mask") (tstamp fca3cba9-4408-4520-a0d5-aeee7f11dc16))
  (model "${KIPRJMOD}/L201011MS02Q.stp"
    (offset (xyz 0 0 1.7))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
