(footprint "SMB_L4.4-W3.6-LS5.4-RD" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -4) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 602e7aa6-8b46-42b9-b898-d5badde02f7e)
  )
  (fp_text value "SMB_L4.4-W3.6-LS5.4-RD" (at 0 4) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 124b3dad-40a6-43e1-b2ab-cf937caa831a)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a9e6cf22-3f8e-4cfc-9d3b-f7f3400b8fc0)
  )
  (fp_line (start -2.75 -1.88) (end 2.74 -1.88)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 40b3d5cd-a45d-477a-9ca7-1e12bb1bb8ad))
  (fp_line (start -2.75 1.89) (end 2.74 1.89)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 945f2e79-4019-420d-9932-66a94fcd255a))
  (fp_line (start -1.02 -1.88) (end -1.02 1.89)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp ae8a0141-18e3-45e2-8a1f-04473f98c03e))
  (fp_line (start -0.38 -0.88) (end -0.38 0.89)
    (stroke (width 0.25) (type solid)) (layer "F.SilkS") (tstamp fd1add3c-6daf-437c-b2de-ee5d590f0922))
  (fp_line (start -0.37 0) (end -0.26 0)
    (stroke (width 0.25) (type solid)) (layer "F.SilkS") (tstamp ad0e0ec8-7a25-48aa-a97f-5b28cb7369d9))
  (fp_line (start -0.26 0) (end -0.33 0)
    (stroke (width 0.25) (type solid)) (layer "F.SilkS") (tstamp 99fd52cf-6053-46b2-bbd6-a370f4ceec05))
  (fp_line (start -0.26 0) (end 0.63 -0.88)
    (stroke (width 0.25) (type solid)) (layer "F.SilkS") (tstamp f5470007-2170-4f4b-9d7e-29daa9632a66))
  (fp_line (start 0.63 -0.88) (end 0.63 0.89)
    (stroke (width 0.25) (type solid)) (layer "F.SilkS") (tstamp 776f3aa2-e116-411e-a957-7f22e0eafdbe))
  (fp_line (start 0.63 0.89) (end -0.26 0)
    (stroke (width 0.25) (type solid)) (layer "F.SilkS") (tstamp 2d1f8ade-99c6-44e6-9f95-51ae056d351f))
  (fp_line (start 1.27 0) (end -0.77 0)
    (stroke (width 0.25) (type solid)) (layer "F.SilkS") (tstamp 26e68a1f-89b6-4b76-8a13-824a60c195e3))
  (fp_line (start 2.74 -1.88) (end 2.74 -1.3)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp b9cc7490-7e15-4c75-893b-d0f369b21b55))
  (fp_line (start 2.74 1.89) (end 2.74 1.3)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 71c6d6a1-6cde-4a41-ae89-6f022ab51216))
  (fp_circle (center -2.7 1.8) (end -2.67 1.8)
    (stroke (width 0.06) (type solid)) (fill none) (layer "F.Fab") (tstamp acac94b4-72b3-45dc-ae77-ef2c0a2e65d2))
  (pad "1" smd rect (at -2.54 0) (size 2.05 2.24) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 8fc41225-84cf-4860-b3e4-08618e45c088))
  (pad "2" smd rect (at 2.54 0) (size 2.05 2.24) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 9be467ef-e09f-45a8-b77b-68fd92686236))
  (model "${KIPRJMOD}/3d models/SMB_L4.4-W3.6-LS5.4-RD.step"
    (offset (xyz 0 -0 -0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
